Smoke And Carbon Alarm Record

Records alarm locations, specifications and operational checks, supporting evidence that required smoke and carbon monoxide protections exist before occupation begins.

Record installation, condition, testing and corrective work. This is a landlord management record, not an electrical installation certificate or fire risk assessment. For Welsh dwellings, required smoke alarms must work, be connected to the electrical supply and interlinked with the other required mains smoke alarms on every storey. Extra alarms do not remove that minimum.
Dwelling address landlord or agent and contract reference: ____________________________
___________________________________________________________________________
Occupation date: _________ Person checking: _____________________________________
___________________________________________________________________________
Number of storeys including basements and other relevant areas: _______________________

Smoke alarms
	Storey and location
	Make model expiry
	Mains interlink test and result

	________________
	________________
________________
	________________________
________________________

	________________
	________________
________________
	________________________
________________________

	________________
	________________
________________
	________________________
________________________

	________________
	________________
________________
	________________________
________________________

	________________
	________________
________________
	________________________
________________________



List each required alarm and any additional battery or heat alarm separately. Check positioning and installation against the manufacturer's instructions and relevant competent advice. Test the interlink, not merely the local sounder. Note inaccessible units, expired sensors or failed backup batteries and act promptly.
Additional devices limitations and associated electrical evidence: _______________________
___________________________________________________________________________
Carbon monoxide alarms and follow up
Identify each room containing a gas, oil-fired or solid-fuel combustion appliance and whether a working carbon monoxide alarm is required. Record any statutory exception precisely, including appliances installed by the contract-holder where applicable. Do not import the English exclusion for gas cookers into Welsh requirements. Follow the manufacturer's positioning and replacement instructions.
	Room appliance fuel
	Alarm make expiry location
	Test date result action

	________________
________________
	____________________
____________________
	____________________
____________________

	________________
________________
	____________________
____________________
	____________________
____________________

	________________
________________
	____________________
____________________
	____________________
____________________

	________________
________________
	____________________
____________________
	____________________
____________________



Exceptions relied upon exact reason and legal basis or none: _________________________________
__________________________________________________________________________________

Defects interim safeguards repairs owner deadline and recheck: _______________________________
__________________________________________________________________________________
Instructions demonstrated to contract holder and date: ______________________________________
__________________________________________________________________________________
Next planned check and replacement reminders: _____________
Checker signature: _________________ date: ___________ and follow up completion evidence:
_________________________________________________________________________________

Tell occupiers how to test alarms and report faults without removing or disabling protection. Do not shift installation, maintenance or replacement duties to them. A receipt or demonstration does not make an unsafe dwelling fit. If an alarm indicates fire or possible carbon monoxide, get to safety and follow emergency advice; do not treat a reset as proof the risk has gone.
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